# Class PrinterStateReason

java.lang.Object
javax.print.attribute.EnumSyntax
javax.print.attribute.standard.PrinterStateReason

All Implemented Interfaces:
  `Serializable, Cloneable, Attribute`

public class PrinterStateReason extends EnumSyntax implements Attribute
Class `PrinterStateReason` is a printing attribute class, an enumeration, that provides additional information about the printer's current state, i.e., information that augments the value of the printer's `PrinterState` attribute. Class PrinterStateReason defines standard printer state reason values. A Print Service implementation only needs to report those printer state reasons which are appropriate for the particular implementation; it does not have to report every defined printer state reason.

Instances of `PrinterStateReason` do not appear in a Print Service's attribute set directly. Rather, a `PrinterStateReasons` attribute appears in the Print Service's attribute set. The `PrinterStateReasons` attribute contains zero, one, or more than one `PrinterStateReason` objects which pertain to the Print Service's status, and each PrinterStateReason object is associated with a `Severity` level of `REPORT` (least severe), `WARNING`, or `ERROR` (most severe). The printer adds a `PrinterStateReason` object to the Print Service's `PrinterStateReasons` attribute when the corresponding condition becomes true of the printer, and the printer removes the `PrinterStateReason` object again when the corresponding condition becomes false, regardless of whether the Print Service's overall `PrinterState` also changed.

IPP Compatibility: The string values returned by each individual `PrinterStateReason` and associated `Severity` object's `toString()` methods, concatenated together with a hyphen (`"-"`) in between, gives the IPP keyword value for a `PrinterStateReasons`. The category name returned by `getName()` gives the IPP attribute name.

See Also:
  - Serialized Form

- ## Field Summary

  Fields
  Modifier and Type
  Field
  Description
  `static final PrinterStateReason`
  `CONNECTING_TO_DEVICE`
  The printer has scheduled a job on the output device and is in the process of connecting to a shared network output device (and might not be able to actually start printing the job for an arbitrarily long time depending on the usage of the output device by other servers on the network).
  `static final PrinterStateReason`
  `COVER_OPEN`
  One or more covers on the device are open.
  `static final PrinterStateReason`
  `DEVELOPER_EMPTY`
  The device is out of developer.
  `static final PrinterStateReason`
  `DEVELOPER_LOW`
  The device is low on developer.
  `static final PrinterStateReason`
  `DOOR_OPEN`
  One or more doors on the device are open.
  `static final PrinterStateReason`
  `FUSER_OVER_TEMP`
  The fuser temperature is above normal.
  `static final PrinterStateReason`
  `FUSER_UNDER_TEMP`
  The fuser temperature is below normal.
  `static final PrinterStateReason`
  `INPUT_TRAY_MISSING`
  One or more input trays are not in the device.
  `static final PrinterStateReason`
  `INTERLOCK_OPEN`
  One or more interlock devices on the printer are unlocked.
  `static final PrinterStateReason`
  `INTERPRETER_RESOURCE_UNAVAILABLE`
  An interpreter resource is unavailable (e.g., font, form).
  `static final PrinterStateReason`
  `MARKER_SUPPLY_EMPTY`
  The device is out of at least one marker supply (e.g. toner, ink, ribbon).
  `static final PrinterStateReason`
  `MARKER_SUPPLY_LOW`
  The device is low on at least one marker supply (e.g. toner, ink, ribbon).
  `static final PrinterStateReason`
  `MARKER_WASTE_ALMOST_FULL`
  The device marker supply waste receptacle is almost full.
  `static final PrinterStateReason`
  `MARKER_WASTE_FULL`
  The device marker supply waste receptacle is full.
  `static final PrinterStateReason`
  `MEDIA_EMPTY`
  At least one input tray is empty.
  `static final PrinterStateReason`
  `MEDIA_JAM`
  The device has a media jam.
  `static final PrinterStateReason`
  `MEDIA_LOW`
  At least one input tray is low on media.
  `static final PrinterStateReason`
  `MEDIA_NEEDED`
  A tray has run out of media.
  `static final PrinterStateReason`
  `MOVING_TO_PAUSED`
  Someone has paused the printer, but the device(s) are taking an appreciable time to stop.
  `static final PrinterStateReason`
  `OPC_LIFE_OVER`
  The optical photo conductor is no longer functioning.
  `static final PrinterStateReason`
  `OPC_NEAR_EOL`
  The optical photo conductor is near end of life.
  `static final PrinterStateReason`
  `OTHER`
  The printer has detected an error other than ones listed below.
  `static final PrinterStateReason`
  `OUTPUT_AREA_ALMOST_FULL`
  One or more output areas are almost full (e.g. tray, stacker, collator).
  `static final PrinterStateReason`
  `OUTPUT_AREA_FULL`
  One or more output areas are full (e.g. tray, stacker, collator).
  `static final PrinterStateReason`
  `OUTPUT_TRAY_MISSING`
  One or more output trays are not in the device.
  `static final PrinterStateReason`
  `PAUSED`
  Someone has paused the printer and the printer's `PrinterState` is `STOPPED`.
  `static final PrinterStateReason`
  `SHUTDOWN`
  Someone has removed a printer from service, and the device may be powered down or physically removed.
  `static final PrinterStateReason`
  `SPOOL_AREA_FULL`
  The limit of persistent storage allocated for spooling has been reached.
  `static final PrinterStateReason`
  `STOPPED_PARTLY`
  When a printer controls more than one output device, this reason indicates that one or more output devices are stopped.
  `static final PrinterStateReason`
  `STOPPING`
  The printer is in the process of stopping the device and will be stopped in a while.
  `static final PrinterStateReason`
  `TIMED_OUT`
  The server was able to connect to the output device (or is always connected), but was unable to get a response from the output device.
  `static final PrinterStateReason`
  `TONER_EMPTY`
  The device is out of toner.
  `static final PrinterStateReason`
  `TONER_LOW`
  The device is low on toner.

- ## Constructor Summary

  Constructors
  Modifier
  Constructor
  Description
  `protected`
  `PrinterStateReason(int value)`
  Construct a new printer state reason enumeration value with the given integer value.

- ## Method Summary

  Modifier and Type
  Method
  Description
  `final Class<? extends Attribute>`
  `getCategory()`
  Get the printing attribute class which is to be used as the "category" for this printing attribute value.
  `protected EnumSyntax[]`
  `getEnumValueTable()`
  Returns the enumeration value table for class `PrinterStateReason`.
  `final String`
  `getName()`
  Get the name of the category of which this attribute value is an instance.
  `protected String[]`
  `getStringTable()`
  Returns the string table for class `PrinterStateReason`.

  ### Methods declared in class EnumSyntax

  `clone, getOffset, getValue, hashCode, readResolve, toString`
  Modifier and Type
  Method
  Description
  `Object`
  `clone()`
  Returns a clone of this enumeration value, which to preserve the semantics of enumeration values is the same object as this enumeration value.
  `protected int`
  `getOffset()`
  Returns the lowest integer value used by this enumeration value's enumeration class.
  `int`
  `getValue()`
  Returns this enumeration value's integer value.
  `int`
  `hashCode()`
  Returns a hash code value for this enumeration value.
  `protected Object`
  `readResolve()`
  During object input, convert this deserialized enumeration instance to the proper enumeration value defined in the enumeration attribute class.
  `String`
  `toString()`
  Returns a string value corresponding to this enumeration value.

  ### Methods declared in class Object

  `equals, finalize, getClass, notify, notifyAll, wait, wait, wait`
  Modifier and Type
  Method
  Description
  `boolean`
  `equals(Object obj)`
  Indicates whether some other object is "equal to" this one.
  `protected void`
  `finalize()`
  Deprecated, for removal: This API element is subject to removal in a future version.
  Finalization is deprecated and subject to removal in a future release.
  `final Class<?>`
  `getClass()`
  Returns the runtime class of this `Object`.
  `final void`
  `notify()`
  Wakes up a single thread that is waiting on this object's monitor.
  `final void`
  `notifyAll()`
  Wakes up all threads that are waiting on this object's monitor.
  `final void`
  `wait()`
  Causes the current thread to wait until it is awakened, typically by being notified or interrupted.
  `final void`
  `wait(long timeoutMillis)`
  Causes the current thread to wait until it is awakened, typically by being notified or interrupted, or until a certain amount of real time has elapsed.
  `final void`
  `wait(long timeoutMillis, int nanos)`
  Causes the current thread to wait until it is awakened, typically by being notified or interrupted, or until a certain amount of real time has elapsed.

- ## Field Details

  - ### OTHER

    public static final PrinterStateReason OTHER
    The printer has detected an error other than ones listed below.

  - ### MEDIA_NEEDED

    public static final PrinterStateReason MEDIA_NEEDED
    A tray has run out of media.

  - ### MEDIA_JAM

    public static final PrinterStateReason MEDIA_JAM
    The device has a media jam.

  - ### MOVING_TO_PAUSED

    public static final PrinterStateReason MOVING_TO_PAUSED
    Someone has paused the printer, but the device(s) are taking an appreciable time to stop. Later, when all output has stopped, the `PrinterState` becomes `STOPPED`, and the `PAUSED` value replaces the `MOVING_TO_PAUSED` value in the `PrinterStateReasons` attribute. This value must be supported if the printer can be paused and the implementation takes significant time to pause a device in certain circumstances.

  - ### PAUSED

    public static final PrinterStateReason PAUSED
    Someone has paused the printer and the printer's `PrinterState` is `STOPPED`. In this state, a printer must not produce printed output, but it must perform other operations requested by a client. If a printer had been printing a job when the printer was paused, the `Printer` must resume printing that job when the printer is no longer paused and leave no evidence in the printed output of such a pause. This value must be supported if the printer can be paused.

  - ### SHUTDOWN

    public static final PrinterStateReason SHUTDOWN
    Someone has removed a printer from service, and the device may be powered down or physically removed. In this state, a printer must not produce printed output, and unless the printer is realized by a print server that is still active, the printer must perform no other operations requested by a client. If a printer had been printing a job when it was shut down, the printer need not resume printing that job when the printer is no longer shut down. If the printer resumes printing such a job, it may leave evidence in the printed output of such a shutdown, e.g. the part printed before the shutdown may be printed a second time after the shutdown.

  - ### CONNECTING_TO_DEVICE

    public static final PrinterStateReason CONNECTING_TO_DEVICE
    The printer has scheduled a job on the output device and is in the process of connecting to a shared network output device (and might not be able to actually start printing the job for an arbitrarily long time depending on the usage of the output device by other servers on the network).

  - ### TIMED_OUT

    public static final PrinterStateReason TIMED_OUT
    The server was able to connect to the output device (or is always connected), but was unable to get a response from the output device.

  - ### STOPPING

    public static final PrinterStateReason STOPPING
    The printer is in the process of stopping the device and will be stopped in a while. When the device is stopped, the printer will change the `PrinterState` to `STOPPED`. The `STOPPING` reason is never an error, even for a printer with a single output device. When an output device ceases accepting jobs, the printer's `PrinterStateReasons` will have this reason while the output device completes printing.

  - ### STOPPED_PARTLY

    public static final PrinterStateReason STOPPED_PARTLY
    When a printer controls more than one output device, this reason indicates that one or more output devices are stopped. If the reason's severity is a report, fewer than half of the output devices are stopped. If the reason's severity is a warning, half or more but fewer than all of the output devices are stopped.

  - ### TONER_LOW

    public static final PrinterStateReason TONER_LOW
    The device is low on toner.

  - ### TONER_EMPTY

    public static final PrinterStateReason TONER_EMPTY
    The device is out of toner.

  - ### SPOOL_AREA_FULL

    public static final PrinterStateReason SPOOL_AREA_FULL
    The limit of persistent storage allocated for spooling has been reached. The printer is temporarily unable to accept more jobs. The printer will remove this reason when it is able to accept more jobs. This value should be used by a non-spooling printer that only accepts one or a small number jobs at a time or a spooling printer that has filled the spool space.

  - ### COVER_OPEN

    public static final PrinterStateReason COVER_OPEN
    One or more covers on the device are open.

  - ### INTERLOCK_OPEN

    public static final PrinterStateReason INTERLOCK_OPEN
    One or more interlock devices on the printer are unlocked.

  - ### DOOR_OPEN

    public static final PrinterStateReason DOOR_OPEN
    One or more doors on the device are open.

  - ### INPUT_TRAY_MISSING

    public static final PrinterStateReason INPUT_TRAY_MISSING
    One or more input trays are not in the device.

  - ### MEDIA_LOW

    public static final PrinterStateReason MEDIA_LOW
    At least one input tray is low on media.

  - ### MEDIA_EMPTY

    public static final PrinterStateReason MEDIA_EMPTY
    At least one input tray is empty.

  - ### OUTPUT_TRAY_MISSING

    public static final PrinterStateReason OUTPUT_TRAY_MISSING
    One or more output trays are not in the device.

  - ### OUTPUT_AREA_ALMOST_FULL

    public static final PrinterStateReason OUTPUT_AREA_ALMOST_FULL
    One or more output areas are almost full (e.g. tray, stacker, collator).

  - ### OUTPUT_AREA_FULL

    public static final PrinterStateReason OUTPUT_AREA_FULL
    One or more output areas are full (e.g. tray, stacker, collator).

  - ### MARKER_SUPPLY_LOW

    public static final PrinterStateReason MARKER_SUPPLY_LOW
    The device is low on at least one marker supply (e.g. toner, ink, ribbon).

  - ### MARKER_SUPPLY_EMPTY

    public static final PrinterStateReason MARKER_SUPPLY_EMPTY
    The device is out of at least one marker supply (e.g. toner, ink, ribbon).

  - ### MARKER_WASTE_ALMOST_FULL

    public static final PrinterStateReason MARKER_WASTE_ALMOST_FULL
    The device marker supply waste receptacle is almost full.

  - ### MARKER_WASTE_FULL

    public static final PrinterStateReason MARKER_WASTE_FULL
    The device marker supply waste receptacle is full.

  - ### FUSER_OVER_TEMP

    public static final PrinterStateReason FUSER_OVER_TEMP
    The fuser temperature is above normal.

  - ### FUSER_UNDER_TEMP

    public static final PrinterStateReason FUSER_UNDER_TEMP
    The fuser temperature is below normal.

  - ### OPC_NEAR_EOL

    public static final PrinterStateReason OPC_NEAR_EOL
    The optical photo conductor is near end of life.

  - ### OPC_LIFE_OVER

    public static final PrinterStateReason OPC_LIFE_OVER
    The optical photo conductor is no longer functioning.

  - ### DEVELOPER_LOW

    public static final PrinterStateReason DEVELOPER_LOW
    The device is low on developer.

  - ### DEVELOPER_EMPTY

    public static final PrinterStateReason DEVELOPER_EMPTY
    The device is out of developer.

  - ### INTERPRETER_RESOURCE_UNAVAILABLE

    public static final PrinterStateReason INTERPRETER_RESOURCE_UNAVAILABLE
    An interpreter resource is unavailable (e.g., font, form).

- ## Constructor Details

  - ### PrinterStateReason

    protected PrinterStateReason(int value)
    Construct a new printer state reason enumeration value with the given integer value.
    Parameters:
      `value` - Integer value

- ## Method Details

  - ### getStringTable

    protected String[] getStringTable()
    Returns the string table for class `PrinterStateReason`.
    Overrides:
      `getStringTable` in class `EnumSyntax`
    Returns:
      the string table

  - ### getEnumValueTable

    protected EnumSyntax[] getEnumValueTable()
    Returns the enumeration value table for class `PrinterStateReason`.
    Overrides:
      `getEnumValueTable` in class `EnumSyntax`
    Returns:
      the value table

  - ### getCategory

    public final Class<? extends Attribute> getCategory()
    Get the printing attribute class which is to be used as the "category" for this printing attribute value.

    For class `PrinterStateReason` and any vendor-defined subclasses, the category is class `PrinterStateReason` itself.

    Specified by:
      `getCategory` in interface `Attribute`
    Returns:
      printing attribute class (category), an instance of class `java.lang.Class`

  - ### getName

    public final String getName()
    Get the name of the category of which this attribute value is an instance.

    For class `PrinterStateReason` and any vendor-defined subclasses, the category name is `"printer-state-reason"`.

    Specified by:
      `getName` in interface `Attribute`
    Returns:
      attribute category name